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The flexibility of an online dripper. The performance of UniRam.
Techline™ CV and HCV Hybrid combines the installation flexibility of an online dripper with the superior performance and reliability of Techline™ CV and HCV inline technology. It is designed for demanding residential and commercial landscape applications, including trees, shrubs, hedges, planting beds and challenging or sloped terrain.
Benefits & Features
· Online Dripper Flexibility – Accessories can be easily connected directly to the dripper outlet, providing greater flexibility for different landscape applications.
· Clogging resistance - Large Filtration Area and large flow path cross section – Provides increased protection against clogging and reliable performance in challenging water conditions.
· Pre-Welded Outlet – Provides a secure, leak-free connection between the dripper and tubing.
· Pressure Compensating – Delivers consistent flow and uniform irrigation across varying pressure conditions and long runs.
· Prevents drainage (CV) - The CV (Check-valve) mechanism maintains dripline pressure by preventing drainage from emitters located in low areas, ensuring uniform water distribution. Eliminates the drainage and refill effect, improving irrigation efficiency in pulse irrigation applications.
· Techline CV Reliability – Combines the proven performance and durability of Techline CV inline dripper technology with the flexibility of an online solution.
Applications.
Trees
Shrubs
Hedges
Planting beds
Challenging or sloped terrain.[image: ]
	CV
	 
	 
	 
	 
	 
	 
	 

	Flow rate* (gph)
	Working pressure range
	Water passages dimmensions (width-depth-length (in)
	Filtration area (mm2)
	Constant K
	Exponent* X
	Recommended filtration (micron)/(mesh)
	Shut off pressure (psi

	0.26
	14 - 58 psi
	0.033 x 0.029 x 1.57
	130
	0.26
	0
	130 / 120
	2

	0.42
	
	0.043 x 0.030 x 1.57
	130
	0.42
	0
	200 / 80
	2

	0.61
	
	0.050 x 0.037 x 1.57
	130
	0.61
	0
	200 / 80
	2

	0.92
	
	0.063 x 0.042 x 1.57
	150
	0.92
	0
	200 / 80
	2

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	HCV
	 
	 
	 
	 
	 
	 
	 

	Flow rate* (gph)
	Working pressure range
	Water passages dimmensions (width-depth-length (in)
	Filtration area (mm2)
	Constant K
	Exponent* X
	Recommended filtration (micron)/(mesh)
	Shut off pressure (psi

	0.33
	21 - 58 psi
	0.028 x 0.026 x 1.57
	110
	0.33
	0
	130 / 120
	3.6

	0.53
	
	0.033 x 0.029 x 1.57
	130
	0.53
	0
	130 / 120
	3.6

	0.77
	
	0.043 x 0.030 x 1.57
	130
	0.77
	0
	200 / 80
	3.6




	Dripline Technical data
	
	
	
	

	Inside diameter, (in)
	Wall Thickness, (in)
	Outside diameter, (in)
	Nominal diameter (mm)
	Maximum working pressure, (psi)
	Maximum flushing pressure, (psi)
	Kd

	0.570
	0.045
	0.660
	17 mm
	55
	72
	1.20

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	Dripline Pachage data
	
	
	
	
	

	Inside diameter, (in)
	Wall Thickness, (in)
	Outside diameter, (in)
	Nominal diameter (mm)
	Coil Length, (ft)
	Average Coils Weight (lb)
	Coils on a Pallet, (Units)

	0.570
	0.045
	0.660
	17 mm
	100
	TBD
	TBD

	0.570
	0.045
	0.660
	17 mm
	250
	TBD
	TBD

	0.570
	0.045
	0.660
	17 mm
	500
	TBD
	TBD

	0.570
	0.045
	0.660
	17 mm
	1000
	TBD
	TBD
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Accessories

Straight 3X5 adapter D Elbow 3X5 adapter
Flot 2 adapter ' - Flot 4 adapter
Plug for Hybrid ‘

Spikes / NetBow™
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